# Trac tickets of package Modelica resolved for version 3.2.1

Color coding of "Priority":

low | normal | high | highest

## Component: --MSL-general-- (44 matches)
| Ticket | Summary | Release Notes
--- | --- | --- | ---
| #292 | Remove empty "Diagram(graphics)" annotations |
| #408 | Replace non-standard annotation by standard annotation attribute `groupImage` |
| #439 | Simulation of Modelica.Utilities.Examples.readRealParameterModel usually fails | Simulation of Modelica.Utilities.Examples.readRealParameterModel no longer requires a specific current directory; instead relies on new loadResource function in ModelicaServices.
| #457 | Garbage in a lot of annotations in MSL 3.2 and MSL 3.1. |
| #465 | Test before the publication of MSL |
| #513 | Illegal tokens in MSL 3.2 | Corrected the number format according to the specification.
| #518 | MSL causes exponential time lookup |
| #528 | Discourage usage of "wildcard imports" |
| #569 | Missing ModelicaStandardLibrary.pdf | Removed link to no-longer generated PDF document.
| #579 | Unknown annotation `Window` present in MSL - remove or specify? |
| #593 | Non-input/parameter expressions for dimensions in function context |
| #747 | Rename `__Dymola_NumberOfIntervals` to `Interval` | Converted `__Dymola_NumberOfIntervals` to `Interval`
| #748 | Replace `__Dymola_InlineNoEvent` to the new standard equivalent |
| #753 | Remaining issues in MSL 3.2.1 trunk |
| #773 | All functions w/o own icon should extend from Modelica.Icons.Function |
| #777 | Typos in MSL documentation |
| #786 | Replace `__Dymola_*` by the new standard equivalents |
| #799 | Complete definition of initialisation of executable models |
| #819 | Redundant use of constrainedby |
| #823 | Clean up examples |
| #838 | HTML doc typos |
| #842 | What is the meaning of Evaluate=true in a type definition? |
| #844 | Non-sense annotation numbers |
| #846 | Removal of empty equation sections |
| #850 | Library contains a number of files of unspecified format (.mos) | The functionality used in the conversion scripts is described in more detail. Note that conversions are only needed for models using MSL 2 or MSL 1.
| #860 | Enumeration-Integer comparison |
| #864 | replaceable extension in ObsoleteModelica3 |
| #929 | Wrong position of external library annotation |
| #947 | Additional Boolean vector functions, improvement to some existing ones |
| #955 | Import using fully-qualified identifiers |
| #1007 | Optimize png file sizes |
| #1021 | Restructure C-Sources directory so that it is according to Modelica specification |
| #1058 | Wrong Modelica web address http://www.Modelica.org |
| #1096 | Redesigned MSL icons. |
| #1114 | Regression testing for MSL 3.2.1 |
| #1124 | It's used incorrectly in ComplexMath | Incorrect use of "it's" in documentation corrected.
| #1132 | Release MSL 3.2.1 |
| #1177 | Missing function icon inheritance |
| #1180 | Quantities of sensor outputs |
| #1185 | Re-enable the visual identifiaction of obsolete models again |
| #1203 | Parameters in examples do not have a binding equation (only a start value) |
| #1207 | Adapting initialization of pre(vc) values for non-discrete Real variables vc |
| #1213 | Empty vs. generated package documentation |
| #1223 | Use of conditionally enabled components |
## Component: --TaskForce:Tables-- (3 matches)
| Ticket | Summary | Release Notes
| #129 | Dymola-specific functions in MSL (Tables and Utilities) | Dymola specific C-code (tables) have been replaced by an open source implementation shipped with MSL under Resources\C-Sources
| #1103 | New open source tables: readTableData relies on appropriate sorting |
| #1146 | New open source tables: minimum number of points needed |
## Component: Blocks (60 matches)
| Ticket | Summary | Release Notes
| #76 | Problems with tables and external functions in MSL |
| #338 | No cleanup of CombiTimeTable at simulation stop | Memory allocated by the Table blocks was not freed after model termination. This has been fixed.
| #451 | Unspecified realString(y, 1, 0) function still present in annotations inside several libraries. |
| #472 | TimeTable |
| #529 | Add new `RateLimiter` block to MSL |
| #566 | TimeTable error, if first timepoint not zero |
| #604 | Modelica.Blocks.Logical |
| #628 | Proposal for enhancement in Blocks.Tables.CombiTable1D,1Ds,2D and Blocks.Sources.CombiTimeTable | New feature of CombiTimeTable block: Optionally, the table values are not interpolated but the hold during the table points
| #644 | FixedDelay() function issue |
| #645 | Missing order annotation |
| #676 | Blocks.Math.Mean has invalid sample function |
| #697 | Error with using min as component name |
| #708 | typos in Modelica.Blocks.Type doc string |
| #745 | Icon for Greater misleading when flipped |
| #751 | Modelica.Blocks.Continuous.LimIntegrator limitsAtInit implmentation |
| #759 | Block Icons |
| #772 | Duplicated code in Add3? |
| #774 | Modelica.Blocks.Discrete.FirstOrderHold has bugs |
| #785 | URIs in file names |
| #787 | LimIntegrator ignores output limits when gain is negative |
| #790 | Invalid use of pre in Blocks.Logical.TriggeredTrapezoid |
| #797 | ChebyshevI initializes array in a weird way |
| #824 | Modelica.Blocks.MathBoolean.MultiSwitch is overconstrained at initialisation |
| #826 | Array parameters in Modelica.Blocks |
| #827 | if-equation with assert() on one branch in Modelica.Blocks.Nonlinear.Limiter |
| #835 | HTML doc typos in Modelica.Blocks |
| #857 | HTML doc typo in Modelica.Blocks.Sources.CombiTimeTable |
| #858 | Physical quantity of Modelica.Blocks.Sources.CombiTimeTable.t_min and t_max |
| #859 | HTML doc error in Modelica.Blocks.Sources.CombiTimeTable |
| #865 | Multiple equations for pre(x) at initialisation |
| #900 | add and product blocks marked as obsolete but still used all over the place |
| #935 | Modelica.Blocks.Math.RootMeanSquare might fail |
| #939 | Modelica.Blocks.Continuous.LimPID with dangling parameters |
| #941 | Modelica.Blocks.Math.MultiSwitch is overconstrained at initialisation |
| #943 | Unnecessary lower bound duration(min=Modelica.Constants.small) |
| #963 | Blocks.Math.Mean: Order of when-equations relevant => rewrite as algorithm! |
| #976 | Remove reference in doc of the now obsolete ConvertAllUnits |
| #987 | Limiter (and LimPID) does not treat limits literally |
| #1022 | Tables: CombiTimeTable with single row and positive start time |
| #1028 | Tables: CombiTimeTable with spline interpolation and linear extrapolation |
| #1031 | Tables: CombiTimeTable with spline interpolation and periodic extrapolation |
| #1039 | Tables: CombiTimeTable with spline interpolation and borderline slopes |
| #1067 | Evaluation of new OpenSourceTables |
| #1072 | Wrong output of OnDelay, if input is true during initialization | Bug fixed in Blocks.MathBoolean.OnDelay (if u=true at initialization, the output y was wrongly set to false for the rest of the time)
| #1075 | Icon of BooleanStep gives the wrong impression if startValue = true | Icon of BooleanStep improved, so that the icon resembles the value of parameter startValue (= false: up step; = true: down step)
| #1090 | ContinuousDerivative Interpolation of OpenSourceTables is wrong |
| #1091 | How to use usertab.c with New OpenSource Tables |
| #1098 | Add cosine sources to MSL | Added new cosine block and voltage sources
| #1102 | How to include Open Source Tables in MSL |
| #1110 | New open source tables: No caching of tables |
| #1136 | Guard debug-messages with a flag |
| #1137 | CombiTables: Empty table fill(0.0, 0, 2) raises an assertion |
| #1138 | Unused variables in Table functions |
| #1143 | Shallow copying of array in Tables |
| #1169 | initial condition for Modelica.Blocks.Math.Mean |
| #1174 | ModelicaStandardTables: Text files with additional line breaks fail |
| #1175 | Unspecified format of tables text files |
| #1178 | OpenSourceTables: Evaluation of table file name |
| #1199 | Modelica.Blocks.Sources.CombiTimeTable with periodic extrapolation not backward compatible |
| #1214 | Missing documentation of Blocks.Types.Init |
## Component: C-Sources (10 matches)
| Ticket | Summary | Release Notes
| #420 | Modelica/Resources/C-Sources does not export symbols |
| #889 | Include error in ModelicaInternal.c |
| #973 | ModelicaUtilities.h misses ModelicaVFormatMessage / ModelicaVFormatError |
| #1032 | Data type of valueStart |
| #1104 | Merging ModelicaInternal.c |
| #1149 | Compiler warnings on win32_dirent.c |
| #1150 | CombiTable1Ds gives different results when multiple instances are used in MSL 3.2.1 beta1 |
| #1151 | Locale-specific reading of files in new tables | Avoid the locale dependency of string to number conversion in C-Sources
| #1155 | Binaries in the Modelica Standard Library |
| #1206 | OpenSourceTables: size(...) in external C function |
## Component: Complex* (3 matches)
| Ticket | Summary | Release Notes
| #585 | Replace non-standard annotation `__Dymola_Protection(hideFromBrowser=true)` |
| #663 | Complex components re and im should probably be replaceable |
| #969 | Amplitude of variables in Electrical.QuasiStationary library |
## Component: Constants (1 match)
| Ticket | Summary | Release Notes
| #706 | proper defintion of Modelica.Constants.small and eps |
## Component: Electrical.Analog (13 matches)
| Ticket | Summary | Release Notes
| #471 | Typo in Modelica.Electrical.Analog.OpAmp |
| #485 | Invalid argument to delay in Modelica.Electrical.Analog.Lines.TLine2 and Modelica.Electrical.Analog.Lines.TLine3 | The models TLine2 and TLine3 were improved according to the Modelica Specification. The variable TD was changed into a parameter since it only depends on parameters.
| #507 | Ineffective call to smooth in Modelica.Electrical.Analog.Basic.OpAmp | Meaningless smooth operator removed in Modelica.Electrical.Analog.Basic.OpAmp. Smooth() was used on the parameter scope.
| #508 | Modelica.Electrical.Analog.Examples.HeatingNPN_OrGate relies on special Dymola specific treatement of constants | Dymola specific constant handling changed to a more general one. constant Modelica.SIunits.Capacitance CapVal=0; changed to parameter Modelica.SIunits.Capacitance CapVal=0;
| #543 | Colors are wrong in annotations for Diode models (and maybe Sources too). | Wrong colours of icons in Modelica.Electrical.Analog changed
| #544 | output connection for Electrical Power Sensor is wrong color, badly routed |
| #717 | Thyristor and GTO issues | The icon of the ideal GTO model from Electrical.Analog was corrected. The documentation of the IdealThyristor and the IdealGTO models were improved. The example CharacteristicThyristors was improved by adding not regular fire signals to show several cases of useage.
| #971 | Initialisation fix r5954 breaks backward compatibility. |
| #1011 | Singular transfomer model if L1=L2=M | Transformer equations changed to handle the case L1=L2=M. A test model for that case was included into ModelicaTest
| #1045 | Use equation-section in M_Transformer | Variable Lm in model M_Transformer changed into parameter. Functionality of the model moved from algorithm section to equation section.
| #1059 | Electrical.Lines.Oline_weg is a duplicate of Oline without HeatPort | Old models OLine_weg and ULine_weg removed (Electrical.Analog)
| #1060 | Electrical.Analog.Examples.MUX2x1 and RAM have no documentation | Documentation added for MUX2x1 and RAM in Electrical.Digital
| #1198 | Capacitor symbol is non-standard |
## Component: Electrical.Digital (10 matches)
| Ticket | Summary | Release Notes
| #460 | Bad/confusing name of component |
| #637 | References to files in Modelica.Electrical.Digital.Memories | file path corrected in Electrical.Digital in order to make memory models work
| #703 | MSL uses bad relations (enum == integer) | Naming of logical values corrected according to specification in Electrical.Digital. Now locial values like L.'O' instead of integers are used.
| #817 | delayTable in InertialDelaySensitive should either be removed or be constant | internal variable delayTable[:,:] removed
| #972 | Algebraic loop when using Integer(...) | Integer(x_delayed) = integer(delay(Integer(x), delayTime)); changed into x_delayed = LogicValues[integer(delay(Integer(pre(x)), delayTime))];in order to avoid an algebraic loop in the models Multiplexer, FlipFlop, FullAdder, Counter3 and Counter from package MSL Electrical.Digital.Examples.
| #998 | Digital.Multiplexers.MUX2x1 uses each on non-array elements | In model Electrical.Digital.Multiplexers.MUX2x1 the keyword each was removed at the instantiation of the variable inertialDelaySensitive since this variable is a scalar.
| #999 | Wrong type of default value in Electrical.Digital.Sources.Table | In Electrical.Digital.Sources.Table an integer value was assigned to an enumeration. This integer was changed into a logical value.
| #1001 | Integer in array of enumeration in Digital.Examples.RAM | Typo corrected in Digital.Examples.RAM. Logical variables had integer values. These were changed to logical ones.
| #1016 | Error in Electrical.Digital when running Dymola2014 Beta in pedantic mode | Setting of initial values revised. Only that array component [n] of the array auxiliary gets an initial value by setting D.Interfaces.Logic auxiliary_n(start=L.'U', each fixed=true); instead of giving the whole array an inital value. This avoids overspecifying of inital value setting.
| #1205 | Digital.Memories.DLATRAM: "when initial() ..." vs "if initial() ..." in algorithm clause | Changed when initial() to if initial() in Modelica.Electrical.Digital.Memories.DLATRAM and Modelica.Electrical.Digital.Memories.DLATROM and changed algorithm section to equation section in Modelica.Electrical.Digital.Sources.Clock
## Component: Electrical.Machines (8 matches)
| Ticket | Summary | Release Notes
| #568 | Modelica.Electrical.Machines.BasicMachines.Components.BasicTransformer has unused signals |
| #570 | PartialBasicMachine not backwards compatible from 3.1 to 3.2 |
| #611 | Functions in Modelica.Electrical.Machines.SpacePhasors.Functions use public constants |
| #642 | Weird connect equations present in MSL3.2 and some user models |
| #872 | Electrical.Machines.Sensors do not provide sensible unit but just Real instead |
| #982 | Difference between `CurrentController` and `DqController` not clear from documentation |
| #983 | New components are missing test models |
| #1003 | Bug in propagation of turnsratio in Machines |
## Component: Electrical.MultiPhase (3 matches)
| Ticket | Summary | Release Notes
| #463 | Update Multiphase examples with stop time |
| #1013 | phase orientation of multiphase sources is wrong for even number of phases |
| #1070 | activePower not inlined | Defined the relationship of the dimensions of the input arguments v and i in the declaration instead of an assert in the algorithm section, to simplify inlining of the function (if a tool supports only inlining of functions with one statement)
## Component: Electrical.QuasiStationary (3 matches)
| Ticket | Summary | Release Notes
| #1089 | Parameter m is not propagated correctly | Missing propagation of parameter m in Star and Delta of QuasiStationary.MulitPhase.Basic fixed
| #1099 | Bug fix for default phase angles of quasi stationary multi phase sources | Bug fix of default phase angles of quasi stationary multi phase voltage and current sources
| #1173 | Syntax error in Modelica.Electrical.QuasiStationary.MultiPhase.Sensors.PowerSensor |
## Component: Electrical.Spice3 (9 matches)
| Ticket | Summary | Release Notes
| #607 | Error in Q_PNPBJT model in MSL.Electrical.Spice3 | Handling of the TBJT parameter in Electrical.Spice3.Q_PNPBJT improved in order to be able to distinguish between Q_PNPBJT and Q_NPNBJT. Setting the TBJT parameter to 1 the model Q_NPNBJT is used, setting it to -1 the Q_PNPBJT model is used.
| #715 | Unassigned variable in Modelica.Electrical.Spice3.Internal.Mos.MosModelLineParams record | Given the variable Real m_surfaceStateDensityIsGiven a startvalue because it hasn't had any value before. The variable is obsolete and only part of the library because of backwards compatibility. Anyway it will be removed in the next version with conversion scripts.
| #769 | New obsoleted models added but why? | Improved models in the Spice3 library were added. The old versions of these models cannot be removed because of backwards compatibility.
| #770 | functions should extend from function icon class |
| #782 | Missing icons for packages, functions and records | extends for the icon definitions added
| #810 | Spice3 connector is unbalanced | Unbalanced InductiveCouplePin was split into two connectors. One output connector and one input connector. The former potential variable L is now, depending on the type of connector, either an input variable or an output variable but no potential variable any longer. So the two new connectors are balanced with one potential variable and one flow variable.
| #869 | Record reference is not constant even though all its members are | Record SpiceConstants C changed from a variable to a parameter since all its members are parameters
| #930 | Undefined protected variable in diodeNoBypassCode function | Fixed an Error in Spice3.Internal.Diode.diodeNoBypassCode. Line m_dCurrent := out_cc.m_dCurrent; added because m_dCurrent did not have any value before.
| #994 | m_capgd not defined in mosCalcNoBypassCode | Several function in Electrical.Spice3 did not specify all outputs. This is corrected now. A second issue that was solved is that the record Modelica.Electrical.Spice3.Internal.Bjt.bjtRenameParameters contained parameters. now the whole record is a parameter and the keyword parameter inside the record is deleted.
## Component: Fluid (39 matches)
| Ticket | Summary | Release Notes
| #205 | Bug in Modelica.Fluid.Examples.IncompressibleFluidNetwork |
| #233 | Divison by zero when useLumpedPressure is enabled in pipe model |
| #247 | Inconsistent use of the variable ''vs'' in component DynamicPipe when nParallel > 1 |
| #250 | Simple fluid models do not initialize properly |
| #323 | Check usage of regRoot2 throughout the library |
| #358 | incomplete path in Fluid.Examples.HeatExchanger.BaseClass.WallConstProps |
| #417 | Out-commented model "`SpecificInternalEnergy`" in `Senors.mo` |
| #495 | Error in Modelica.Fluid.Utilities.regFun3 |
| #500 | dead link |
| #542 | Problem with initialization of Fluid models |
| #549 | missingInnerMessage in Fluids.System is tool-specific. |
| #562 | Missing appropriate min-max attributes in Media implementations |
| #575 | Check of `ControlledPump` fails |
| #596 | Non-visible spliceFunction in Modelica/Fluid/Pipes.mo |
| #627 | Non-identical inherited components in Fluid.Fittings |
| #646 | PartialPump uses undefined Medium.saturationProperty |
| #649 | PartialTwoPhaseMedium redeclares functions with wrong input dimensions |
| #680 | Simulation of Modelica.Fluid.Examples.HeatingSystem fails |
| #693 | Modelica.Fluid.Valves.ValveIncompressible and regRoot2 |
| #722 | Replace obsoleted model `DynamicPipe` by alternatives via conversion script |
| #736 | Use of m_flow_small, m_flow_turbulent and dp_small |
| #737 | replicated code in Sensor package (for m_flow_small) |
| #739 | MassFlowSource_T with 2 ports does not balance flow among port[1]+port[2] |
| #741 | Heat exchanger example invalid |
| #754 | Out-commented classes present |
| #836 | Undefined annotation choicesAllMatching still appears in a few places | Corrected the name of tool vendor annotation.
| #848 | regFun3 does not always define its outputs |
| #852 | Modelica.Fluid.Examples.AST_BatchPlant.BaseClasses.TriggeredTrapezoid is duplicate, unused & invalid |
| #912 | Typing issues for HeatExchangerSimulation via Modelica.Fluid.Examples.HeatExchanger.BaseClasses.BasicHX |
| #916 | Remove non-standard annotation `editButton` |
| #936 | Provide docu and examples for PipeOnePhaseHT and PipeTwoPhaseHT |
| #948 | Absolute sensors assign potentially invalid values to port variables |
| #953 | Missing inner stateGraphRoot in Modelica.Fluid.Examples.ControlledTankSystem.ControlledTanks |
| #974 | Errors in homotopy implementations in MSL 3.2.1 |
| #989 | Revert to assert function rather than use of blunt print statements |
| #1068 | Illegal uses of conditional components in Fluid.Vessels | PartialLumpedVessel: Made the conditional component VesselPortsData non-conditional and instead set the size of this array to zero, incase use_portsData is false
| #1112 | MoistAir: Temperature validity range seems to be wrong |
| #1168 | unexpected warning from "Modelica.Fluid.Examples.TraceSubstances.RoomCO2" |
| #1222 | ModelicaTest.Fluid.TestComponents.Vessels.TestInitialization does not initialize |
## Component: Fluid.Dissipation (13 matches)
| Ticket | Summary | Release Notes
| #330 | import statement not resolve in annotation |
| #498 | Wrong type in record dp_twoPhaseOverall_IN_con |
| #501 | Inconsistency in function TwoPhaseDensity() |
| #502 | Unit in FluidDissipation correlation |
| #679 | function inheritance from non-function |
| #718 | Illegal characters in Modelica/Fluid/Dissipation.mo |
| #793 | Failure in dialog annotation of record Geometry | Fixed typo in dialog annotation name of record `Geometry`
| #904 | Missing h in documentation of dp_curvedOverall |
| #914 | Momentum pressure loss for two phase fluids | Calculation of momentum pressure loss for two phase fluids corrected.
| #996 | function kc_overall has undefined output |
| #1135 | spelling of Prandtl in Fluid.Dissipation | Fixed a typo in the name "Prandtl".
| #1188 | Discontinues v_smooth in dp_edgedOverall_MFLOW |
| #1212 | FluidDissipation in Modelica.Fluid.Dissipation |
## Component: Icons (1 match)
| Ticket | Summary | Release Notes
| #1191 | Wrong prefix for TypeComplex and SignalBus |
## Component: Magnetic.FluxTubes (3 matches)
| Ticket | Summary | Release Notes
| #525 | Type for MagneticPort potential could be better |
| #584 | Parameters declared as variables |
| #942 | Modelica.Magnetic.FluxTubes.Examples.SolenoidActuator.ComparisonQuasiStationary is overconstrained at initialisation |
## Component: Magnetic.FundamentalWave (7 matches)
| Ticket | Summary | Release Notes
| #589 | Bug in calculation of core conductance in FundamentalWave library | Calculation of core conductance in `FundamentalWave` corrected.
| #881 | Salient record needs to have replaceable components |
| #990 | Extend FundamentalWave library to phase numbers greater than three |
| #1107 | HTML errors in FundamentalWave |
| #1129 | SinglePhaseInductance/MultiPhaseInductance: Missing initial conditions |
| #1216 | TpmOperational in Modelica.Magnetic.FundamentalWave.BasicMachines.SynchronousInductionMachines.SM_PermanentMagnet |
| #1226 | FundamentalWave: orientation of rotor currents |
## Component: Math (13 matches)
| Ticket | Summary | Release Notes
| #550 | Strange description string for Modelica.Math.Vectors.length |
| #582 | Wrong annotation for visibility feature used |
| #629 | Error in documentation for Modelica.Math.atan3? |
| #636 | Not all Math functions are derived from Function icon |
| #678 | Blocks.Math.RectifiedMean: typo in annotation |
| #719 | Library annotations in LAPACK |
| #801 | Type errors in function realSchur |
| #918 | Bug in calculating eigenvectors with "eigenValues/dgeev" |
| #928 | Bug in calling dgeevx from LAPACK |
| #931 | Unnecessary declarations of builtin functions as external C libraries in Math |
| #960 | Undefined type used within annotation for LAPACK function / Inefficiencies |
| #970 | Doc example of Matrices.solve2 |
| #1004 | Test an Integer whether it is a power of 2 |
## Component: Mechanics.MultiBody (33 matches)
| Ticket | Summary | Release Notes
| #130 | Small typo in: Modelica.Mechanics.MultiBody.Sensors |
| #242 | Missing each qualifier for modifiers in MultiBody. | Added missing each-prefixes to modifications
| #255 | Error in Revolute's handling of non-normalized axis of rotations |
| #400 | Should MultiBody.Types.Color be an Integer[3] or Real[3]? |
| #509 | fullRobot animation |
| #510 | fullRobot animation |
| #511 | scalarToColor algorithm fails |
| #517 | Dialog annotation of colors in Modelica.Mechanics.MultiBody |
| #534 | MultiBody UsersGuide |
| #572 | Support URI in the shapeType definition |
| #583 | Misplaced `min=` argument in annoation section |
| #653 | Images of `Mechanics` documentation are not stored according to the convention. |
| #674 | HTML tag error in Modelica.Mechanics.MultiBody.Joints |
| #675 | HTML doc typos in Modelica.Mechanics.MultiBody |
| #749 | Unexpected selection of time states when using Rotor1D |
| #781 | Regarding quantity="Position" in MSL |
| #803 | GravityTypes referred to as Integer |
| #804 | Duplicate modifier in ConstrainUniversalJoint |
| #820 | Syntax error in Modelica/Mechanics/MultiBody/Sensors.mo |
| #845 | Superfluous multiple inheritance in Modelica.Mechanics.MultiBody.Visualizers.Advanced.Shape |
| #875 | Physical quantity "Angles" nowhere defined |
| #911 | Modelica.Mechanics.MultiBody.Frames.Internal.maxWithoutEvent |
| #923 | Wrong semantics of binding equation for parameters with fixed=false in MSL |
| #944 | Modelica.Mechanics.MultiBody.Examples.Constraints.* |
| #945 | Modelica.Mechanics.MultiBody.Examples.Loops.Fourbar2 is overconstrained at initialisation |
| #956 | possible wrong array size in Modelica.Mechanics.MultiBody.Visualizers.Colors.ColorMaps.jet |
| #1002 | MultiBody.Joints.Constraints.UniversalJoint uses == on Real |
| #1037 | Different units in output 'w' and internal sensoroutput 'w' in BasicAbsoluteAngularVelocity |
| #1113 | MultiBody.Parts.FixedRotation: Input possible in disabled menu | MultiBody.Parts.FixedRotation: Minor issue fixed that allowed inputs in disabled menu depending on RotationType
| #1116 | Warning from jointRRR | Initialisation of `jointRRR` corrected by adding a missing `each`.
| #1144 | Assertions of MultiBody.Examples.Loops.Utilities.GasForce2 |
| #1194 | Non-backward compatible definition of external CAD shapes |
| #1200 | Visualization of torus |
## Component: Mechanics.Rotational (6 matches)
| Ticket | Summary | Release Notes
| #615 | What is the meaning of phi_nominal in Mechanics.Rotational.PartialCompliantWithRelativeStates |
| #701 | Poor default values in PartialFriction |
| #821 | Missing dialog annotation for Modelica.Mechanics.Rotational.Sources.Speed.f_crit | Missing `Dialog` annotation added .
| #876 | Sensors should use sensible units/quantities as output rather than just real |
| #927 | UTF-8 BOM in Rotational.mo |
| #1162 | Component defined twice in Modelica.Mechanics.Rotational.Components.Clutch |
## Component: Mechanics.Translational (8 matches)
| Ticket | Summary | Release Notes
| #446 | Negative displacements of translational springs should be permitted |
| #526 | Length parameters incorrectly declared as distance |
| #707 | Wrong definition of "s" in Mechanics.Translational.Components.SupportFriction |
| #734 | Wrong experiment annotation for Modelica.Mechanics.Translational.Examples.Accelerate |
| #840 | Comment typo of Modelica.Mechanics.Translational.Components.Brake |
| #873 | Modelica.Mechanics.Translational.Components.ElastoGap c and d parameters need types | Enhanced `ElastoGap` parameters by usage of SIunits.
| #1121 | Bad modeling in Modelica.Mechanics.Translational.Examples.HeatLosses? |
| #1156 | reinit in MassWithStopAndFriction is in algorithm section which is no longer allowed | Rewrote model MassWithStopAndFriction so that reinit is used in an equation and not in an algorithm section (which is no longer allowed in Modelica 3.2 rev 2)
## Component: Media (58 matches)
| Ticket | Summary | Release Notes
| #139 | fluidConstants.triplePointXxxx are declared but not set for ideal gases |
| #179 | Include inverse annotation for Media T_phX functions |
| #397 | Ask for adding function isentropicEnthalpy in Media MoistAir |
| #482 | Modelica.Media.Air.MoistAir leads to illegal Modelica lookup! |
| #488 | spliceFunction is used from the builtin environment but is not defined in the Modelica Specification! |
| #505 | Illegal modification of inherited element in Modelica.Media.Water.WaterIF97_base |
| #530 | Wrong description for reference_s in PartialLinearFluid |
| #539 | Invalid examples in Modelica.Media |
| #547 | WaterIF97: allow p<p_triple in region 2 |
| #557 | Illegal redeclare of non-replaceable parameter standardOrderComponents in Modelica.Media |
| #564 | Regularization of cp/h_pTX_der |
| #580 | Unknown annotation `InlineNoEvent` present in MSL - remove or specify? |
| #595 | Missing "replaceable" declaration |
| #600 | Specific internal energy in PartialSimpleIdealGasMedium |
| #625 | Syntax errors in Modelica Standard Library |
| #631 | Error discovered in Essothermal oil viscosity |
| #640 | Use of protected classes in MSL (2) |
| #691 | Problem with implementation of setState functions in Media.IdealGases.Common.MixtureGases |
| #692 | Global integer constant for thermal conductivity calculation method in gas media |
| #710 | Bug in Modelica.Media.Examples.MixtureGases? |
| #731 | Use of partial package SingleGasNasa |
| #732 | Modification of FluidLimits record |
| #735 | Modification of FluidLimits record required |
| #792 | Wrong assert for region 2 of IF97 |
| #794 | molarMass in PartialTwoPhaseMedium is partial |
| #798 | dtofph3 has logic error |
| #806 | Incompressible medica functions lack derivative annotations | Improved Modelica.Media.Incompressible with analytic derivatives
| #818 | output of saturationTemperature_derp should be of type DerTemperatureByPressure |
| #890 | Missing argument to Internal.solve |
| #903 | velocityOfSound and isentropicExponent in ideal Gases lacking annotation on being differentiable |
| #924 | MolarMass instantiated from a partial package |
| #950 | Modelica.Media.Air.MoistAir.isentropicEnthalpy not working |
| #952 | Modelica.Media.Air.MoistAir.isentropicEnthalpyApproximation not working |
| #964 | Corrupted WaterIF97 medium models basing on WaterIF97_fixedregion |
| #995 | waterBaseProp_pT contains undefined outputs |
| #1017 | Fix usage of GenerateEvents and Inline annotations in Modelica.Fluid |
| #1040 | Inconsistent treatment of event generation and phase output in Water model |
| #1041 | Undeclared function "LogVariable()" used in IF97_Utilities | Removed use of undeclared function LogVariable from Modelica.Media.Water.IF97_Utilities.BaseIF97.Inverses.dofpt3
| #1053 | Moving test models from Modelica.Media to ModelicaTest | Moved test models from Modelica.Media to ModelicaTest
| #1055 | Base class FluidConstants is replaceable |
| #1069 | Type error in Media.Air.SimpleAir | Readability of vector expression improved in Media.Air.SimpleAir
| #1080 | Model Modelica.Media.Examples.Tests.Components.PartialTestModel changed in a non-backwards compatible way |
| #1092 | PartialMedium changed in a non-backwards compatible way | Modelica.Media.Interfaces.PartialMedium: Choices definition re-introduced as obsolete element in order that Media are backwards compatible (has been previously moved one level up to Media.Interfaces.Choices)
| #1093 | MoistAir function argument names changed in a non-backwards compatible way | Renamed function input arguments of two MoistAir functions to the names from MSL 3.2 for backwards compatibility
| #1100 | Should derivative=sublimationPressureIce_der be removed in r6326? |
| #1105 | Inclusion of MoMoLib in trunk |
| #1106 | Modelica.Media conformance to the specification |
| #1109 | Combining different FluidConstants type in RealGasMoistAir is not possible |
| #1115 | Fix description strings in Modelica.Media |
| #1122 | Adding yet another Complex record seems wrong |
| #1130 | 3.2.1 Beta1 fails on MapleSim Parser |
| #1161 | Error in Modelica.Media.Air.DryAirNasa |
| #1164 | assert(true, "message") will never be evaluated |
| #1171 | Validity range of dynamic viscosity function for ideal gases |
| #1187 | Bug in calculation of thermal conductivity for mixture gases |
| #1209 | Wrong definition of inverse annotation in T_ph of Modelica.Media.Incompressible |
| #1210 | Specific energy u of Modelica.Media.Incompressible.Examples.Glycol47 is slightly wrong |
| #1217 | Issues with ReferenceMoistAir (isentropicEnthalpy, Inverses.p_dTX |
## Component: Resources (1 match)
| Ticket | Summary | Release Notes
| #1141 | Missing newline when printing to terminal | Streams.print: Missing automatic newline after a call of print(..) added in Resources\C-Sources\ModelicaInternal.c
## Component: SIunits (5 matches)
| Ticket | Summary | Release Notes
| #688 | Add Complex Units (Magnetic) |
| #779 | SIunits type for generic nondimensional ratio is missing | New type "PerUnit" was added.
| #795 | Physical types in Modelica.SIunits should not have start, min, or max values. |
| #898 | Wrong Modelica.SIunits.Conversions.{to_cm2, from_cm2} |
| #1192 | Modelica.SIunits.ComplexXXX is wrongly defined as record, must be operator record |
## Component: StateGraph (6 matches)
| Ticket | Summary | Release Notes
| #353 | Error in Modelica.StateGraph.StateGraphRoot annotation |
| #450 | Unspecified boolean(x) function present in annotations inside StateGraph library. |
| #946 | initial conditions for Modelica.Stategraph.Examples.* |
| #954 | Capital letters for classes in Modelica.StateGraph.Examples.Utilities |
| #997 | Misleading documentation in StateGraph.StateGraphRoot |
| #1208 | Structural change makes discrete variable t_start continuous and then pre(t_start) is not allowed in initial equation section |
## Component: Thermal.HeatTransfer (6 matches)
| Ticket | Summary | Release Notes
| #830 | Physical unit of Thermal.HeatTransfer.Celsius.TemperatureSensor.T |
| #949 | Documentation of FixedHeatFlow and PrescribedHeatFlow |
| #1063 | Correct docu-html in Modelica.Thermal.HeatTransfer.Components.Convection | Html error corrected in documentation of Thermal.HeatTransfer.Components.Convection ("<" instead of "<")
| #1073 | Illegal use of conditional component in Thermal.HeatTransfer.Examples.ControlledTemperature | Illegal use of conditional component in Thermal.HeatTransfer.Examples.ControlledTemperature corrected by replacing it with a non-conditional variable reference
| #1125 | Modelica.Thermal.HeatTransfer.Sensors in 3.2.1beta1 are not backward compatible |
| #1204 | degF displayed twice |
## Component: UsersGuide (5 matches)
| Ticket | Summary | Release Notes
| #198 | Name of components in MSL not according to naming conventions |
| #221 | Convention Guide recommends obsolete tags for mark up and emphasizing |
| #610 | Are functions allowed to start with a non-capital letter? |
| #896 | HTML doc typo in Modelica.UsersGuide.ReleaseNotes.Version_3_0 |
| #1211 | Different copyright notice |
## Component: Utilities (5 matches)
| Ticket | Summary | Release Notes
| #443 | `readRealParameterModel` will fail if not the correct working directory is set |
| #639 | Use of protected classes in MSL |
| #761 | Wrong external declaration in getEnvironmentVariable |
| #831 | Function findLast crashes when defining 'startIndex' |
| #1078 | improvements of Modelica.Utilities |
## Component: _ModelicaReference (5 matches)
| Ticket | Summary | Release Notes
| #565 | ModelicaReference contains removed operators |
| #670 | Missing functions need to be added to `ModelicaReference` |
| #756 | The homotopy operator is missing in ModelicaReference |
| #802 | Add new standard operator `rooted()` to ModelicaReference | `Connections.*()` operators were added to the `ModelelicaReference` documentation.
| #988 | Add new standard annotations to ModelicaReference | New Spec 3.2Rev2 annotations were added to the ModelicaReference.
## Component: _ModelicaServices (4 matches)
| Ticket | Summary | Release Notes
| #811 | Synchronise version numbering of `ModelicaServices` and `Complex` with MSL |
| #919 | Default implementation of ModelicaServices |
| #920 | Remove variants of ModelicaServices and only ship the default version |
| #1172 | ModelicaServices.Animation.Surface should extend Modelica.Utilities.Internal.PartialModelicaServices.Animation.PartialSurface | Added missing extends clause to ModelicaServices.Animation.Surface
## Component: _ModelicaTest (5 matches)
| Ticket | Summary | Release Notes
| #372 | Issue with ModelicaTest.Fluid.TestComponents.Machines.TestWaterPumpDefault |
| #437 | Simulation of ModelicaTest.Fluid.TestComponents.Pipes.DynamicPipeWithNominalLaminarFlow fails1 |
| #788 | Update ModelicaTest library so it does not use ObsoleteModelica3 components | Removed dependency on ObsoleteModelica3 in ModelicaTest.
| #805 | Continuous_InitialState uses wrong enumeration |
| #958 | ModelicaTest.Fluid.Dissipation uses integers as enumerations |