# Trac tickets of package Modelica resolved for version 3.2.1 build 3

Color coding of "Priority":

low | normal | high | highest

## Component: --MSL-general-- (7 matches)

| Ticket | Summary | Release Notes
--- | --- | --- | ---
| #807 | Replace deprecated `rooted` by `Connections.rooted` | Replaced deprecated "rooted" by "Connections.rooted"
| #1134 | correct usage of units in MSL? |
| #1245 | Is assignment of a derived record instance to a base record instance allowed? | Casting of records is not allowed. A record constructor was integrated in wrapper functions.
| #1614 | Remove bad LinePattern.None from MSL | Removed bad LinePattern.None from MSL
| #1681 | Release test MSL 3.2.1+build.3-rc1 |
| #1683 | Upgrade MSL 3.2.1+build.3 to MSL 3.2.2 ? |
| #1694 | Rendering of bitmaps | Bitmap annotations corrected
## Component: --RegressionTesting-- (1 match)
| Ticket | Summary | Release Notes
| #1392 | Specifiy setup for MSL Regression Testing |
## Component: --TaskForce:Tables-- (3 matches)
| Ticket | Summary | Release Notes
| #1307 | Small 2d-tables causes issues | Added support of 2D tables that actually degrade to 1D tables for Modelica Standard Tables
| #1619 | Erroneous Table Interpolation when applying startTime | Fixed the detection of time events of the CombiTimeTable with non-zero start time of the Modelica Standard Tables
| #1630 | Cannot compile ModelicaStandardTables on trunk | Moved declaration of HAVE_MAT_INT64_T / HAVE_MAT_UINT64_T from source to header (ModelicaMatIO.[ch])
## Component: Blocks (7 matches)
| Ticket | Summary | Release Notes
| #1302 | Invalid Icon annotation in Modelica.Blocks.MathInteger.MultiSwitch. |
| #1448 | Default component name for class "Not" is "nor1" |
| #1477 | Issue with Modelica.Blocks.Examples.BooleanNetwork1 |
| #1571 | Falling parameter in Slew Rate Limiter | Corrected parameter limit of SlewRateLimter.
| #1617 | Incorrect (?) min value for "Falling" in SlewRateLimiter |
| #1664 | Strange integer(precision) annotation in Blocks.Math.MultiSwitch | Replaced wrong "integer(precision)" by "precision" in annotations of blocks Blocks.Math.MultiSwitch and StateGraph.Temporary.NumericValue
| #1701 | Blocks.Types.InitPID has typo in comment string |
## Component: C-Sources (11 matches)
| Ticket | Summary | Release Notes
| #1263 | Tables: GCC error if ANSI C is forced | Fixed ANSI-C compliance of Modelica Standard Tables
| #1264 | Tables: Text files with Windows line endings cannot be read on Linux | Fixed reading table files with Windows line endings on Linux (ModelicaStandardTables.c)
| #1269 | Tables: Update Matio Library | Updated matio library to official release 1.5.2 (ModelicaMatIO.[ch])
| #1273 | ModelicaStrings.c does not compile on dSPACE targets | Fixed compilation of ModelicaStrings on dSPACE DS1006
| #1465 | Discontinuous change in Modelica.Blocks.Tables.CombiTable2D | Fixed the linear and bilinear extrapolation of the bivariate Akima-splines of the Modelica Standard Tables
| #1494 | Tables: More precise error message if dimensions do not match | Improve the error message in case of trailing numbers in external table text files of the Modelica Standard Tables
| #1508 | ModelicaInternal_print to terminal not available if NO_FILE_SYSTEM is set | Fixed ModelicaInternal_print (for Modelica.Utilities.Streams.print) to also output the string to terminal on platforms where a file system is not present (e.g. on dSPACE or xPC)
| #1556 | Critical sections | Fixed multi-threaded access of global variables in C-Sources
| #1569 | ModelicaMatIO.c not fully platform independent | Avoid platform dependency of SIZEOF_LONG (and other) in sources of the Modelica Standard Tables
| #1580 | File reading works differently depending on OS | Fixed platform dependency of ModelicaInternal_readFile and ModelicaInternal_readLine
| #1682 | Long initialisation for CombiTimeTable using v7 MAT-files | Modelica Standard Tables: Fixed poor performance of readMatTable for MATLAB MAT-files with compressed array streams and large (> 1e5) number of rows
## Component: Electrical.Analog (8 matches)
| Ticket | Summary | Release Notes
| #1240 | Typo in comment-strings of HeatingNMOS and HeatingPMOS kk2 parameter |
| #1289 | ChuaCircuit has uninteresting StopTime |
| #1300 | Misplaced Placement annotation in Electrical.Analog.Ideal |
| #1393 | Typo in diagram layer of Modelica.Electrical.Analog.Sources.TableCurrent |
| #1475 | Missing comment for parameter Modelica.Electrical.Analog.Basic.M_Transformer.Lm |
| #1519 | Wrong stop time in ChuaCircuit |
| #1562 | switch2.tSwitch should be (fixed=true) in Modelica.Electrical.Analog.Examples.SwitchWithArc |
| #1563 | unfixed startvalues in Modelica.Electrical.Analog.Examples.AD_DA_conversion | Digital.Sources.Pulse, DA_Converter, AD_Converter: Adding missing fixed=true values for discrete-time variables
## Component: Electrical.Digital (1 match)
| Ticket | Summary | Release Notes
| #1564 | unfixed initial value in Modelica.Electrical.Digital.Sources.Clock |
## Component: Electrical.Machines (5 matches)
| Ticket | Summary | Release Notes
| #1446 | Non conform Modelica.Electrical.Machines.Losses.Friction |
| #1474 | Bugs in transformers: wrong sign of secondary power calculation & orientation of secondary components | Fixed wrong sign of secondary power calculation and wrong orientation of secondary resistor and stray inductor
| #1504 | Modelica.Electrical.Machines.Examples.SynchronousInductionMachines.SMPM_Inverter missing 'each' for smpm.ir.fixed |
| #1570 | inconsistent initial System for Modelica.Electrical.Machines.Examples.SynchronousInductionMachines.SMEE_LoadDump |
| #1579 | Wrong temperature propagation in transformer ambient | Fixed wrong temperature propagation in thermal ambient
## Component: Electrical.Spice3 (6 matches)
| Ticket | Summary | Release Notes
| #1308 | Missing StopTime |
| #1404 | Remove experiment annotation from subcircuits in Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder | The experiment annotations (StopTime, Interval) in Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder.FOURBIT Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder.NAND Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder.ONEBIT Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder.TWOBIT were removed. Also the documentation of Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder was improved.
| #1427 | Uninitialized local variables in Modelica.Electrical.Spice3.Internal.Mos.mos2CalcNoBypassCode used |
| #1428 | Uninitialized local variable temp in Modelica.Electrical.Spice3.Internal.Bjt.bjtNoBypassCode used |
| #1566 | unfixed start values in Modelica.Electrical.Spice3.Sources.I_pulse and Modelica.Electrical.Spice3.Sources.V_pulse | Spice3.Sources.I_pulse/.V_pulse: Added missing fixed=true initialization for discrete variable
| #1639 | Translation fails for Modelica.Electrical.Spice3.Examples.Spice3BenchmarkFourBitBinaryAdder |
## Component: Fluid (11 matches)
| Ticket | Summary | Release Notes
| #1306 | Incompatible change in MSL 3.2.1 for Modelica.Fluid.Machines.BaseClasses.PartialPump | introduced a dummy parameter show_NPSHa to the PartialPump model, in order to improve backwards compatibility (show_NPSHa was removed in MSL 3.2.1)
| #1309 | AST_BatchPlant.Test.* lack experiment annotation |
| #1352 | wall model in Modelica.Fluid.Examples.HeatExchanger.BaseClasses.BasicHX |
| #1471 | HeatExchanger.BaseClasses.BasicHX: Wrong parameter values |
| #1527 | Parametrization of HeatExchangerSimulation model in Modelica.Fluid |
| #1560 | Type error in BatchPlant_StandardWater |
| #1582 | Min/Max Assertion in 3 Examples from Modelica.Fluid.Examples.AST_BatchPlant.Test |
| #1601 | Wrong calculation of Reynolds number for non-circular pipes |
| #1633 | Modelica.Fluid.Examples.HeatExchanger.BaseClasses.WallConstProps Mistake |
| #1656 | Fluid.Pipes.BaseClasses.WallFriction.PartialWallFriction.pressureLoss_m_flow not backward compatible |
| #1738 | each on scalar in DynamicPipe | Removed erroneous use of 'each' in Fluid.
## Component: Fluid.Dissipation (7 matches)
| Ticket | Summary | Release Notes
| #1188 | Discontinuous v_smooth in dp_edgedOverall_MFLOW | Corrected the transition between laminar and turbulent region
| #1335 | Problem with StepSmoother | Corrected Stepsmoother function to avoid numerical problems
| #1343 | Should Modelica.Fluid.Dissipation.PressureLoss.Bend.dp_curvedOverall_DP and similar functions have Inline=false? | Dissipation functions have either annotation Inline=false or Inline=true
| #1350 | Issue in Fluid.Dissipation function | Introduced a numerical expansion for laminar and transition conditions to avoid numerical errors due to rounding.
| #1421 | Sign error in derivative of SmoothPower | Erroneous derivative of SmoothPower corrected for x≤-adeltax
| #1549 | Error in straight pipe heat transfer model for laminar flow | Fixed error in straight pipe heat transfer model for laminar flow
| #1631 | Calculation of A2 in dp_curvedOverall_MFLOW and dp_curvedOverall_DP | Factor A2 was corrected in range >0.55-0.7.
## Component: Magnetic.FundamentalWave (1 match)
| Ticket | Summary | Release Notes
| #1531 | Incomplete sentence in Contact documentation | Removed broken sentence from documentation
## Component: Math (4 matches)
| Ticket | Summary | Release Notes
| #1285 | Dimension of Xk in continuousRiccatiIterative and discreteRiccatiIterative | Avoid dependency of input array dimension on output array dimension in continuousRiccatiIterative and discreteRiccatiIterative
| #1286 | Typos in LU_solve2 |
| #1589 | No default output for sigma in function Modelica.Math.Matrices.singularValues | Matrices.singularValues: if zero-dimension A, sigma=0 is returned (was undefined)
| #1661 | Extra argument in dgelsx | Fix function arguments and documentation of Math.Matrices.LAPACK.dgelsx and dgelsx_vec
## Component: Mechanics.MultiBody (5 matches)
| Ticket | Summary | Release Notes
| #1361 | UserDefinedGravityAcceleration redeclared with modifier mue |
| #1376 | Invalid Icon annotations in MultiBody. |
| #1402 | Small typo in colorMapToSvg example |
| #1452 | Huge gravitySphereDiameter in PointGravityWithPointMasses2 | Decreased Mechanics.MultiBody.Examples.Elementary.PointGravityWithPointMasses2.world.gravitySphereDiameter
| #1565 | EngineV6: incorrect experiment stop time or wrong mention of stop time in documentation | MultiBody.Examples.EngineV6/EngineV6_analytic: Documentation improved regarding StopTime
## Component: Mechanics.Rotational (4 matches)
| Ticket | Summary | Release Notes
| #1375 | Example "Modelica.Mechanics.Rotational.Examples.GenerationOfFMUs" |
| #1403 | Fix description string in Modelica.Mechanics.Rotational.Components.AngleToTorqueAdaptor |
| #1523 | Move block + MultiBody model can give issues with index reduction |
| #1554 | Modelica.Mechanics.Rotational.Components.LossyGear | LossyGear: #1554 fixed (Modelica.Mechanics.Rotational.Components.LossyGear): Added missing unit and description texts to all public variables.
## Component: Mechanics.Rotational3D (2 matches)
| Ticket | Summary | Release Notes
| #1315 | Is mount axis in MovingActuatedDrive correct? |
| #1605 | Non-evaluated axis parameters in MultiBody.Rotational3D | Added Evaluate=true annotation to axes parameters of Mounting1D, Rotor1D, Bevel1D
## Component: Mechanics.Translational (3 matches)
| Ticket | Summary | Release Notes
| #1331 | wrong connection color for support flanges |
| #1353 | Color of connection line from Interfaces.Support |
| #1437 | Modelica.Mechanics.Translational.Examples.InitialConditions |
## Component: Media (11 matches)
| Ticket | Summary | Release Notes
| #1014 | Dymola-specific code in MSL 3.2.1 | Tool-specific workaround removed.
| #1390 | Cyclical definition in Modelica.Media.Incompressible.TableBased | Removed circular type definition for Temperature type
| #1422 | Uninitialized var in function Modelica.Media.Water.IF97_Utilities.waterBaseProp_dT used | Fixed unitialized variable aux_cv in function Modelica.Media.Water.IF97_Utilities.waterBaseProp_dT
| #1442 | Possibly incorrect algorithm in Modelica.Media.Interfaces.PartialSimpleIdealGasMedium |
| #1530 | PartialSimpleIdealGasMedium uses different offsets in BaseProperties and in specificInternalEnergy | Fixed ticket #1350, wrong offset for u in PartialSimpleIdealGasMedium.
| #1583 | Undefined return value in Polynomials_Temp.integral |
| #1593 | wrong parameter declaration in MSL model |
| #1629 | Record declaration clashes with function definition. | Media.Common.IF97BaseTwoPhase: Changed equation phase=0 to phase(start=0) to avoid an error when the record is returned from a function
| #1650 | Derivative function has mismatched arguments names | Bug in derivative function arguments in Modelica.Media fixed
| #1675 | Modelica.Media.package.mo still has __Dymola_choicesAllMatching | Removed erroneous __Dymola annotation that was somehow not fixed simultaneously in trunk and this branch.
| #1679 | Circular reference in Modelica.Media.Air.MoistAir.PsychrometricData | Circular Reference bug in Modelica.Media fixed
## Component: Thermal.HeatTransfer (2 matches)
| Ticket | Summary | Release Notes
| #1576 | Icon for Modelica.Thermal.HeatTransfer.Fahrenheit.FixedTemperature needs update |
| #1577 | Icons for PrescribedTemperature and TemperatureSensor need update |
## Component: _ModelicaServices (1 match)
| Ticket | Summary | Release Notes
| #1457 | Relative path as arg to loadResource() | Changed docu of loadResource(): input can be URI or local absolute path name (relative path name is not guaranteed)
## Component: _ModelicaTest (3 matches)
| Ticket | Summary | Release Notes
| #1333 | Uses of conditional components in ModelicaTest.MultiBody |
| #1529 | Assert may have no effect for ModelicaTest.Media.TestAllProperties.PartialMediumFunctions |
| #1607 | Annotation in wrong place in usertab tests |