last-generated=2024-06-02
statistics-initialization=
{
  "nonlinear": "1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0",
  "numerical Jacobians": "0"
}
statistics-simulation=
{
  "linear": " ",
  "nonlinear": " ",
  "number of continuous time states": "3",
  "numerical Jacobians": "0"
}
time=[0e+00, 1e+00]
mulMul.ports_a[1].m_flow=[1e+00, 1e+00]
mulMul.ports_b[1].m_flow=[-1e+00, -1e+00]
mulMul.m_flow_nominal=[3e+00, 3e+00]
mulMulCom.ports_a[1].m_flow=[1e+00, 1e+00]
mulMulCom.ports_b[1].m_flow=[-1e+00, -1e+00]
mulMulCom.m_flow_nominal=[3e+00, 3e+00]
mulSin.ports_a[1].m_flow=[1e+00, 1e+00]
mulSin.port_b.m_flow=[-3e+00, -3e+00]
mulSin.m_flow_nominal=[3e+00, 3e+00]
sinMul.port_a.m_flow=[3e+00, 3e+00]
sinMul.ports_b[1].m_flow=[-1e+00, -1e+00]
sinMul.m_flow_nominal=[3e+00, 3e+00]
pas.port_a.m_flow=[1e+00, 1e+00]
