## FCSys.Characteristics.'C+'.Graphite

C+ graphite

### Information

Assumptions:

1. Constant specific volume (i.e., incompressible and without thermal expansion)

Additional notes:

- The data for this species is for C rather than C+, with the exception of specific mass.
- The radius is from http://en.wikipedia.org/wiki/Carbon. See also http://en.wikipedia.org/wiki/Van_der_Waals_radius.
- The default specific volume (`v = U.cc*m/(2.210*U.g)`) is of pyrolytic graphite at 300 K according to [Incropera2002, p. 909]. Other forms are (Ibid., also at 300 K) are:
  - Amorphous carbon: `v = U.cc*m/(1.950*U.g)`
  - Diamond (type IIa): `v = U.cc*m/(3.500*U.g)`

For more information, please see the Characteristic package.

Extends from BaseClasses.Characteristic (Package of thermodynamic and diffusive properties).