## FCSys.UsersGuide.Glossary

Extends from Modelica.Icons.Information (Icon for general information packages).

### Package Content

Name | Description
--- | ---
'configuration' | (noun) a species in a certain phase within a subregion
'continuity' | (noun) resistivity to axial compression or material storage during transport [M N-1 T-1]
'density' | (noun) amount of material per volume [N L-3]
'equivalent current' | (noun) rate of supply of a reactant required to support the electrical load at 100% utilization of that reactant [N T-1]
'exchange' | (noun) transfer of a conserved quantity among configurations within a region
'fluidity' | (noun) reciprocal of dynamic viscosity [L T M-1]
'Gibbs potential ' | (noun) specific Gibbs energy [L2 M N-1 T-2]
'lineic ' | adjective that indicates the quotient of the following quantity and its associated length [× L-1]
'massic' | adjective that indicates the quotient of the following quantity and its associated mass [× M-1]
'particle number' | (noun) number of particles [N]
'specific' | adjective that indicates the quotient of the following quantity and its associated particle number [× N-1]
'thermal independity' | (noun) extent to which an exchange of thermal energy between species causes or requires a temperature difference [T]
'translational Nusselt number ' | (noun) correction to Newton's law of viscous shear for the shape of the flow profile [1]
'transport' | (noun) transfer of a conserved quantity between adjacent subregions
'volumic' | adjective that indicates the quotient of the following quantity and its associated volume [× L-3]

## FCSys.UsersGuide.Glossary.'configuration'

(noun) a species in a certain phase within a subregion

### Modelica definition

    class 'configuration'
      "(noun) a species in a certain phase within a subregion"

    end 'configuration';

## FCSys.UsersGuide.Glossary.'continuity'

(noun) resistivity to axial compression or material storage during transport [M N-1 T-1]

### Information

See ζ().

### Modelica definition

    class 'continuity'
      "(noun) resistivity to axial compression or material storage during transport [M N-1 T-1]"

    end 'continuity';

## FCSys.UsersGuide.Glossary.'density'

(noun) amount of material per volume [N L-3]

### Information

Synonyms: concentration, molar concentration, number density

Note that mass per volume is volumic mass (see massic).

### Modelica definition

    class 'density'
      "(noun) amount of material per volume [N L-3]"

    end 'density';

## FCSys.UsersGuide.Glossary.'equivalent current'

(noun) rate of supply of a reactant required to support the electrical load at 100% utilization of that reactant [N T-1]

### Modelica definition

    class 'equivalent current'
      "(noun) rate of supply of a reactant required to support the electrical load at 100% utilization of that reactant [N T-1]"

    end 'equivalent current';

## FCSys.UsersGuide.Glossary.'exchange'

(noun) transfer of a conserved quantity among configurations within a region

### Modelica definition

    class 'exchange'
      "(noun) transfer of a conserved quantity among configurations within a region"

    end 'exchange';

## FCSys.UsersGuide.Glossary.'fluidity'

(noun) reciprocal of dynamic viscosity [L T M-1]

### Information

See η().

### Modelica definition

    class 'fluidity'
      "(noun) reciprocal of dynamic viscosity [L T M-1]"

    end 'fluidity';

## FCSys.UsersGuide.Glossary.'Gibbs potential '

(noun) specific Gibbs energy [L2 M N-1 T-2]

### Modelica definition

    class 'Gibbs potential '
      "(noun) specific Gibbs energy [L2 M N-1 T-2]"

    end 'Gibbs potential ';

## FCSys.UsersGuide.Glossary.'lineic '

adjective that indicates the quotient of the following quantity and its associated length [× L-1]

### Modelica definition

    class 'lineic '
      "adjective that indicates the quotient of the following quantity and its associated length [× L-1]"

    end 'lineic ';

## FCSys.UsersGuide.Glossary.'massic'

adjective that indicates the quotient of the following quantity and its associated mass [× M-1]

### Modelica definition

    class 'massic'
      "adjective that indicates the quotient of the following quantity and its associated mass [× M-1]"

    end 'massic';

## FCSys.UsersGuide.Glossary.'particle number'

(noun) number of particles [N]

### Information

Note that particle number is equivalent to amount of material due to the system of units (see the Units package).

### Modelica definition

    class 'particle number'
      "(noun) number of particles [N]"

    end 'particle number';

## FCSys.UsersGuide.Glossary.'specific'

adjective that indicates the quotient of the following quantity and its associated particle number [× N-1]

### Modelica definition

    class 'specific'
      "adjective that indicates the quotient of the following quantity and its associated particle number [× N-1]"

    end 'specific';

## FCSys.UsersGuide.Glossary.'thermal independity'

(noun) extent to which an exchange of thermal energy between species causes or requires a temperature difference [T]

### Information

See ν().

### Modelica definition

    class 'thermal independity'
      "(noun) extent to which an exchange of thermal energy between species causes or requires a temperature difference [T]"

    end 'thermal independity';

## FCSys.UsersGuide.Glossary.'translational Nusselt number '

(noun) correction to Newton's law of viscous shear for the shape of the flow profile [1]

### Modelica definition

    class 'translational Nusselt number '
      "(noun) correction to Newton's law of viscous shear for the shape of the flow profile [1]"

    end 'translational Nusselt number ';

## FCSys.UsersGuide.Glossary.'transport'

(noun) transfer of a conserved quantity between adjacent subregions

### Modelica definition

    class 'transport'
      "(noun) transfer of a conserved quantity between adjacent subregions"

    end 'transport';

## FCSys.UsersGuide.Glossary.'volumic'

adjective that indicates the quotient of the following quantity and its associated volume [× L-3]

### Information

Example: volumic mass [M L-3]

### Modelica definition

    class 'volumic'
      "adjective that indicates the quotient of the following quantity and its associated volume [× L-3]"

    end 'volumic';